**CSE SWITCH**CSE#show running-config

Building configuration...

Current configuration : 1286 bytes

!

version 12.1

no service timestamps log datetime msec

no service timestamps debug datetime msec

service password-encryption

!

hostname CSE

!

enable secret 5 $1$mERr$hx5rVt7rPNoS4wqbXKX7m0

!

spanning-tree mode pvst

!

interface FastEthernet0/1

description "CSE Interface"

!

interface FastEthernet0/2

!

interface FastEthernet0/3

!

interface FastEthernet0/4

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

!

interface FastEthernet0/24

!

interface Vlan1

no ip address

shutdown

!

interface Vlan25

description "COnnected TO CSE"

mac-address 0090.2b44.4101

ip address 192.168.10.2 255.255.255.128

!

banner motd ^CCSE Switch Console^C

!

line con 0

password 7 0822455D0A16

login

!

line vty 0 4

password 7 0822455D0A16

login

line vty 5 15

password 7 0822455D0A16

login

!

end

**ECE SWITCH**

ECE#show running-config

Building configuration...

Current configuration : 1288 bytes

!

version 12.1

no service timestamps log datetime msec

no service timestamps debug datetime msec

service password-encryption

!

hostname ECE

!

enable secret 5 $1$mERr$hx5rVt7rPNoS4wqbXKX7m0

!

spanning-tree mode pvst

!

interface FastEthernet0/1

description "ECE Interface"

!

interface FastEthernet0/2

!

interface FastEthernet0/3

!

interface FastEthernet0/4

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

!

interface FastEthernet0/24

!

interface Vlan1

no ip address

shutdown

!

interface Vlan25

description "COnnected to ECE"

mac-address 00d0.9752.8001

ip address 192.168.10.130 255.255.255.224

!

banner motd ^CECE Switch COnsole^C

!

!

!

line con 0

password 7 0822455D0A16

login

!

line vty 0 4

password 7 0822455D0A16

login

line vty 5 15

password 7 0822455D0A16

login

!

end

**EIE Switch**

EIE#show running-config

Building configuration...

Current configuration : 1288 bytes

!

version 12.1

no service timestamps log datetime msec

no service timestamps debug datetime msec

service password-encryption

!

hostname EIE

!

enable secret 5 $1$mERr$hx5rVt7rPNoS4wqbXKX7m0

!

spanning-tree mode pvst

!

interface FastEthernet0/1

description "EIE Interface"

!

interface FastEthernet0/2

!

interface FastEthernet0/3

!

interface FastEthernet0/4

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

!

interface FastEthernet0/24

!

interface Vlan1

no ip address

shutdown

!

interface Vlan25

description "Connected TO EIE"

mac-address 000a.419c.7301

ip address 192.168.10.162 255.255.255.224

!

banner motd ^CEIE Switch Console^C

!

line con 0

password 7 0822455D0A16

login

!

line vty 0 4

password 7 0822455D0A16

login

line vty 5 15

password 7 0822455D0A16

login

!

end

**IT Switch**

IT#show running-config

Building configuration...

Current configuration : 1284 bytes

!

version 12.1

no service timestamps log datetime msec

no service timestamps debug datetime msec

service password-encryption

!

hostname IT

!

enable secret 5 $1$mERr$hx5rVt7rPNoS4wqbXKX7m0

!

!

!

spanning-tree mode pvst

!

interface FastEthernet0/1

description "IT Interface"

!

interface FastEthernet0/2

!

interface FastEthernet0/3

!

interface FastEthernet0/4

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

!

interface FastEthernet0/24

!

interface Vlan1

no ip address

shutdown

!

interface Vlan25

description "Connected TO IT"

mac-address 00e0.8f4d.2801

ip address 192.168.10.194 255.255.255.224

!

banner motd ^CIT Switch Console^C

!

line con 0

password 7 0822455D0A16

login

!

line vty 0 4

password 7 0822455D0A16

login

line vty 5 15

password 7 0822455D0A16

login

!

end